These files were generated in RS274-X format (embedded apertures)
using CadSoft Eagle 5.2.4:

MicroRC-REV-C             01/09/2009

MicroRC-REV-C.CAD         GenCad Assembly/Mount Data
MicroRC-REV-C.FAB         Fabmaster Assembly/Mount Data
MicroRC-REV-C.MNT         Mount Data TOP side
MicroRC-REV-C.SPT         Solder Paste Mask TOP side
MicroRC-REV-C-TOP.PDF     Top Silkscreen Legend in PDF format

Mount Data Format
-----------------
Generates files for smds on the top and bottom layers wich can be used with mounting machines.
The x and y coordinates (units: mm) of the SMD elements are calculated as mean of maximum
and mimimum value of the smds origin points. The calculated value does not necessarily
fit with the origin point of the part in the layout. The syntax of the output data looks like this:

name x-coord y-coord rotation value package


PCB Layout Contact:
-------------------
Bob Starr
(770) 663-0076
Atlanta, GA USA
mail: robertstarr@comcast.net
http://www.bobstarr.net