<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>74LVX4245
8-Bit Dual Supply Translating Transceiver
with 3-STATE Outputs</description>
<packages>
<package name="74LVX4245">
</package>
</packages>
<symbols>
<symbol name="74LVX4245">
<pin name="VCCB"/>
<pin name="~OE"/>
<pin name="B0"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="VCCA"/>
<pin name="T/~R"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="GND"/>
<pin name="GND1"/>
<pin name="VCCB1"/>
<pin name="GND2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="74LVX4245" prefix="74LVX4245">
<gates>
<gate name="74LVX4245" symbol="74LVX4245"/>
</gates>
<devices>
<device name="" package="74LVX4245">
<connects>
<connect gate="74LVX4245" pin="A0" pad="P$16"/>
<connect gate="74LVX4245" pin="A1" pad="P$17"/>
<connect gate="74LVX4245" pin="A2" pad="P$18"/>
<connect gate="74LVX4245" pin="A3" pad="P$19"/>
<connect gate="74LVX4245" pin="A4" pad="P$20"/>
<connect gate="74LVX4245" pin="A5" pad="P$21"/>
<connect gate="74LVX4245" pin="A6" pad="P$22"/>
<connect gate="74LVX4245" pin="A7" pad="P$23"/>
<connect gate="74LVX4245" pin="B0" pad="P$5"/>
<connect gate="74LVX4245" pin="B1" pad="P$6"/>
<connect gate="74LVX4245" pin="B2" pad="P$7"/>
<connect gate="74LVX4245" pin="B3" pad="P$8"/>
<connect gate="74LVX4245" pin="B4" pad="P$9"/>
<connect gate="74LVX4245" pin="B5" pad="P$10"/>
<connect gate="74LVX4245" pin="B6" pad="P$11"/>
<connect gate="74LVX4245" pin="B7" pad="P$12"/>
<connect gate="74LVX4245" pin="GND" pad="P$24"/>
<connect gate="74LVX4245" pin="GND1" pad="P$25"/>
<connect gate="74LVX4245" pin="GND2" pad="P$13"/>
<connect gate="74LVX4245" pin="T/~R" pad="P$15"/>
<connect gate="74LVX4245" pin="VCCA" pad="P$14"/>
<connect gate="74LVX4245" pin="VCCB" pad="P$1"/>
<connect gate="74LVX4245" pin="VCCB1" pad="P$3"/>
<connect gate="74LVX4245" pin="~OE" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
